**Community Air Monitoring Program**

**Dates: May 20, 2019 to May 24, 2019**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Date** | | **Analysis** |
|  | **Background Corrected Particulate Concentrations (mg/m3)** | | **Response Required?** |
| **Daily Average** | **Daily Max** | **No** |
| **May 20, 2019** | -- | -- | **No** |
| **May 21, 2019** | -- | -- | **No** |
| **May 22, 2019** | -- | -- | **No** |
| **May 23, 2019** | 0.005 | 0.080 | **No** |
| **May 24, 2019** | -- | -- | **No** |

**Air Quality Action Levels**

Background corrected particulate concentration data from the site is compared to particulate action levels. This correction is calculated by subtracting the upwind concentration from the downwind concentration and provides the concentration of particulates being generated by site activities. The specific action levels and their response are as follows:

* Between 0.100 mg/m3 and 0.150 mg/m3 – Particulate suppression techniques instituted.
* Greater than 0.150 mg/m3 – Stop work and reevaluate activities

**Inclement Weather**

Monitoring is not conducted during rain and heavy snow events as precipitation acts as a natural suppressant and prevents the migration of particulates. In addition, moisture can impact the accuracy of the data from the monitors.